page_244

< previous page | page_244 | next page >

Page 244

| Figure 13-6 (cont.) Induction type of overcurrent relay: (B) induction overcurrent electromagnet with torque compensator, and (C) internal connections. |

| Other Types |

| Other relays employing the induction principle use more than one disc and more than one actuating coil. Some use a cylinder in place of one or more discs. Such relays are shown schematically in Fig. 13-8, also shown are their operating characteristics, indicating typical orders of magnitude only. A diagram of the disc type of overcurrent relay previously described is included for comparison. |

< previous page | page_244 | next page >