page_329

< previous page | page_329 | next page >

Page 329

Figure 16-16 (cont.)
Ignitron tube: (C) Circuit of tube controlled by a gas-filled diode (load-current ignition).
(D) circuit of tube controlled by a thyraton (load-current ignition), and (E) circuit of
tube controlled by a capacitor discharge (separately excited ignition) (Courtesy, General
Electric Co.)

< previous page | page_329 | next page >