page_350

< previous page | page_350 | next page >

Page 350

Figure 17-19 (cont.)
The T-90 displays data in large, easy-to-read liquid crystal digits that shine though strong
and clear in high ambient light, including direct sunlight. The display confirms the register
operation. Up to 17 items are available for selection in the display scroll. If the register
should fail, the electronic module can be removed with the memory intact. Or, if the module
should fail, you can put a new module into the existing meter without changing the meter
identification. All electronic modules are identical.

| kilowatt-hour consumption and the floating hand is read for the kilowatt demand. Through a lever protruding from the case, the floating hand is returned to zero each time the meter is read, preparing it to register the maximum demand for the next metering period. This lever is usually locked to prevent tampering. |

| The reading of the floating hand is also transmitted to another set of dials on another register similar to the one measuring consumption. When the lever or plunger is pushed and thus returns the floating hand to zero, it also causes the new maximum demand to be added to the original reading. The new reading provides a means to check and record demand readings. |

< previous page | page_350 | next page >